Parametric Tool for Automated Slot Insulation Insertion in Small-Scale Electric Motor Stator Production

Alen Sebastian  
Institute for Factory Automation and Production Systems (FAPS)  
Friedrich-Alexander-Universität Erlangen-Nürnberg (FAU)

*Abstract*— The increasing trend toward automation in electric motor manufacturing has led to the development of robotic systems for processes such as winding insertion, lamination stacking, and stator assembly. One critical step, slot liner insertion, is typically automated in large-scale production using dedicated Slot Liner insertion machines. However, in small-scale manufacturing, this process is predominantly performed manually due to low production volumes and the impracticality of configuring specialized machines for each variant. This paper presents a flexible and scalable approach by using a parametric funnel in conjunction with a UR 10e robot equipped with a HEX Force-Torque sensor and a RG2 Gripper to insert the slot liner into the stator. The parametric funnel, modeled using CAD, enables rapid adaptation to different stator slot geometries by generating customized insertion tools. This method aims to reduce manual effort, setup time, and cost, making it suitable for low-volume, high-variability production environments. Experimental validation demonstrates the feasibility and repeatability of the proposed system, indicating its potential for improving flexibility in motor manufacturing.

Keywords— Slot Liner Insertion, UR10e Robot, Parametric funnel, low-volume high variability production

# Introduction

Electric motor production is experiencing unprecedented growth to meet the rising demand in various industries. As a result, both the design and manufacturing processes are undergoing continuous optimization. An electric motor generally consists of three main components: the stator, rotor, and housing. The housing is typically produced through pressure die casting, followed by precision machining. The stator and rotor cores are made from laminated electrical steel sheets, which are shaped using either punching or laser cutting methods. These laminations are then assembled using techniques such as riveting or adhesive bonding. Once assembled, slot liners and copper windings are installed in the laminated core. The winding phases are then insulated, formed, and interconnected. The ends of the enameled wires are connected through soldering or welding, followed by processes like bandaging, electrical testing, and impregnation to finalize the stator [1]

This paper focuses on optimizing the slot liner insertion process. In low-voltage electric motors, the slot liner serves two key purposes: it provides electrical insulation for the winding and facilitates effective thermal dissipation. Enhancing the thermal conductivity of the slot liner while retaining its insulating properties can contribute to improved motor efficiency [2]

A close up of a plastic container

AI-generated content may be incorrect.

Fig.1 Image of Stator with slot liner insertions. Elmotec Statomat

Need for Small scale Automation –

* Production of electric motors in small batches is common in industries such as aerospace where electric motors are custom designed based on the specific requirements
* In such a context, implementation of a dedicated slot-liner insertion machine for every stator size and design is not feasible
* Manual insertion is usually done here, which can be:

1. Operator dependent, leading to variability in quality
2. Less scalable and harder to document
3. Prone to errors and physically straining when repeated over long durations

* Automating this task using a general purpose industrial robot (such as UR10e) combined with a parametric tool for different stator sizes can significantly improve:

1. Process repeatability
2. Efficiency and cycle times
3. Flexibility for high variable, low volume production

# State of the Art

## Solutions for large scale production

In state-of-the-art electric motor manufacturing, particularly for distributed windings, advanced slot insulation processes are employed to ensure precise and reliable electrical insulation of the stator slots. One prominent example is the system developed by Schaeffler ELMOTEC STATOMAT, which uses automated machinery to insert specially shaped insulation paper (e.g., U-, O-, B-, or S-shape) into each stator slot. This process involves a sequential combination of creasing, folding, inserting, and cutting the insulation material to exact specifications. The system ensures accurate paper protrusion on both flat surfaces of the stator stack, protecting the copper winding from sharp edges and avoiding interference during insertion. The machines are designed for both small and large series production, offering high adaptability through features such as an automatic empty cycle mechanism to accommodate varying slot geometries. With insertion speeds reaching up to three sleeves per second, the system provides a balance of flexibility, precision, and high throughput, thereby supporting efficiency and scalability for motor production processes [3]

A diagram of a grooving roller

AI-generated content may be incorrect.A machine with a screen and buttons

AI-generated content may be incorrect.In addition to Schaeffler’s ELMOTEC STATOMAT systems, several other industrial manufacturers offer advanced solutions for automated slot insulation in electric motors. **Alliance Winding Equipment** offers machines that form, cuff, and insert insulating materials into stator or rotor slots. These systems integrate cam and servo controls for both speed and precision and allow rapid tooling changes to support multiple lamination types with minimal downtime [4]. **GROB** provides programmable insulation machines with user-friendly operation, offering precise control over insulation length, height, width, and cuff formation—delivering high performance in both accuracy and productivity [5]. **Delta S.R.L.** contributes with slot insulation machines that cut, shape, and insert insulators tailored to the specific slot geometry. These machines support robotic stator handling, quick mold changeovers, and automated height adjustment, making them ideal for high-output production environments.

Fig 2 Dedicated slot liner insertion machine from alliance winding equipments

## Solutions for small scale production

Despite significant advancements in automation, manual insertion of slot liners remains the standard practice in the small-scale manufacture of electric motors.

* In such setups, operators typically cut, fold, and insert the slot liners entirely by hand, or use machines for cutting and folding while performing the insertion manually with simple jigs. This process relies heavily on visual inspection and tactile feedback to ensure proper alignment.
* A metal roller with words

  AI-generated content may be incorrect.However, with the growing demand for electric motors, the need for scalable and streamlined production is increasing. In this context, automation becomes a better alternative—not because manual methods are ineffective, but because they are difficult to integrate into digital workflows, challenging to scale, and not easily documented for consistent reproduction.

Fig 3, 4 grooving module and process adapted from [6]

## Automation Principles

1. **Parametric tooling for flexibility with different variants.** CAD based funnel models are parametrically defined to allow quick adaptation to different slot geometries. Advantages – low cost and low lead times when changing stator configurations
2. **Low-cost automation for small scale production.**The focus is on creating a cost-effective alternative to high end slot liner machines for small scale high variability production. A UR10e robot is used here, due to its balance of affordability, ease of deployment and a user-friendly interface for programming
3. **Mechanically guided precision** - Use of a parametric funnel helps mechanically align theslot liner with the stator slot, minimizing the reliance on sensors or vision systems.
4. **Scope for expansion –** The system architecture, including the force-torque sensor and gripper, supports modular upgrades such as real-time force feedback or adaptive control**.** Potential to integrate vision in future stages. Code and hardware setup remain modular to accommodate future feedback loops or dynamic planning

## Flexibility in automation

* The use of a parametric funnel design enables rapid customization of insertion tools to match different stator slot dimensions.
* Sensor integration (HEX- Force-torque sensor) supports modular feedback capabilities, which would improve the funnel and slot liner insertion process
* An RG2 adaptive gripper allows for flexible grasping of slot liners or funnels, supporting different sizes and insertion techniques without mechanical reconfiguration.
* A grey robot arm with black handles

  AI-generated content may be incorrect.A close-up of a robot

  AI-generated content may be incorrect. The robot, sensor, and gripper combination form a modular, reconfigurable automation cell, well-suited for research environments and evolving production needs.

Fig 5,6 Hex FT sensor and RG2 gripper

## Parametric tools and processes for flexibility enlargement

* The automation setup is designed to adapt to varying stator geometries and slot designs, common in production of electric motors in small batches. This is achieved through modular hardware and a parametric tool design.
* Interchangeable parametric tools – Custom funnels are generated through parametric CAD models, enabling rapid reconfiguration for different stator types. These tools can be easily fabricated through 3D printing.
* **Sensor-Assisted Modularity**
  + The integrated **HEX-E force-torque sensor** actively monitors contact forces during **funnel insertion**, enabling force-based feedback to ensure correct positioning and avoid excessive contact forces or misalignment.
  + This sensor-based interaction enhances robustness during setup and allows the robot to respond to resistance, improving insertion accuracy.
  + The presence of the sensor also makes the system extensible—allowing future integration of **active force-feedback control** during slot liner insertion, enabling more precise and adaptable operation under variable tolerances.

*F. Derivation of consequences*

* **Effectiveness of a mechanically guided system**:  
  The use of a parametric funnel enabled proper alignment of the slot liner even without the implementation of complex sensors such as vision. This confirms that mechanical guidance is a viable method for small batch automation where sensor complexity is undesirable
* **Impact of HEX Force-Torque Sensor**: Using a FT sensor during funnel insertion reduced the risk of over-pressing and misalignment which would otherwise damage the funnel. (add FT to list of abbreviations)
* **Scalability for high variant manufacturing**: The parametric nature of the funnel allows rapid adaptation to different stator geometries. This demonstrates a clear path for scaling the system towards high-variability low volume environments such as prototyping or small batch electric motor production
* **Process sensitivity to slot-liner geometry:** The success of the insertion process was found to\be highly dependent on the profile of the slot liner. If the slot liner is not pre-bent into the exact requirements, it tends to return with the funnel during retraction. This highlights the need for precise slot-liner preparation to ensure a successful insertion process
* **Remaining challenges and future work:** The current system does not automate the full slot liner cycle (grooving, folding, and cutting). Integration of pre-folding tools and a slot liner dispenser mechanism could significantly improve the robustness of the system

# Proposed Parametric Tool and Process

To enable reliable and flexible slot liner insertion in small batch electric motor production, a custom design funnel tool was developed and integrated with a UR10e robot equipped with a RG2 gripper and HEX FT sensor. The funnel serves as a mechanically guided insertion aid that aligns the slot liner with the stator slot. The design is parametric, allowing rapid customization for different stator geometries and insertion requirements.

## Fundamental Tool design

* The tool consists of an **enclosed rectangular body** with an **internal tapered channel** that converges toward the stator slot.

A drawing of a metal object

AI-generated content may be incorrect.

* The inner surface of the funnel features **two gently curved guiding walls**, directing the slot liner into the correct slot while maintaining central alignment
* The central opening ensures that the liner passes through only when aligned, preventing twisting or buckling.
* The **tapered profile** of the funnel not only aligns the slot liner but also **slightly compresses it**, ensuring it holds its shape as it passes into the stator
* The notch in the front of the funnel extrudes to the inner portion of the slot geometry, ensuring that the correct height of the slot-liner with the slot is always maintained (could use more clarity)

A grey object with a hole in the middle

AI-generated content may be incorrect.

* Guide rail on the back of the funnel ensures that the funnel is properly aligned with the slot
* Slots on the sides of the guide rails ensures for tighter insertion of the funnel and it also ensures that the funnel is locked to the stator

A grey rectangular object with a rectangular object in the middle

AI-generated content may be incorrect.

* The mouth of the funnel is intentionally widened to provide a tolerance margin, accommodating slight misalignments during slot liner insertion.
* The tool is lightweight and fabricated using 3D printing, which allows for quick iteration and low-cost customization in small-batch production environments.
* The sides of the tool were made rectangular so that the robot can properly grip the tool. (a side length 0f 2 cm is favorable for proper gripping)
* The tail of the tool was intentionally made longer (50 mm) to obtain a better position for the center of gravity. This ensures that the tool does not tilt forward and causes misalignment with the stator.
* A gap of 1 mm was set between the guide notch and the bottom opening of the funnel so that the funnel insertion is done more smoothly. The ends of the guide notch was also tapered off to prevent the slot liner from coming back with the funnel during funnel removal

A close-up of a metal corner

AI-generated content may be incorrect.

## Selecting of adjustable Parameters

Required parameters:

* Slot-Width
* Slot-Height
* A drawing of a triangle with lines and a point

  AI-generated content may be incorrect.Slot-angle

## Fitting Adjustable parameters for specific use cases

The equations are an exception to the prescribed specifications of this template. You will need to determine whether or not your equation should be typed using either the Times New Roman or the Symbol font (please no other font). To create multileveled equations, it may be necessary to treat the equation as a graphic and insert it into the text after your paper is styled.

Number equations consecutively. Equation numbers, within parentheses, are to position flush right, as in (1), using a right tab stop. To make your equations more compact, you may use the solidus ( / ), the exp function, or appropriate exponents. Italicize Roman symbols for quantities and variables, but not Greek symbols. Use a long dash rather than a hyphen for a minus sign. Punctuate equations with commas or periods when they are part of a sentence, as in:

*a**b* 

Note that the equation is centered using a center tab stop. Be sure that the symbols in your equation have been defined before or immediately following the equation. Use “(1)”, not “Eq. (1)” or “equation (1)”, except at the beginning of a sentence: “Equation (1) is . . .”

## Proposed automation insertion Pipeline

* The word “data” is plural, not singular.
* The subscript for the permeability of vacuum **0, and other common scientific constants, is zero with subscript formatting, not a lowercase letter “o”.
* In American English, commas, semicolons, periods, question and exclamation marks are located within quotation marks only when a complete thought or name is cited, such as a title or full quotation. When quotation marks are used, instead of a bold or italic typeface, to highlight a word or phrase, punctuation should appear outside of the quotation marks. A parenthetical phrase or statement at the end of a sentence is punctuated outside of the closing parenthesis (like this). (A parenthetical sentence is punctuated within the parentheses.)
* A graph within a graph is an “inset”, not an “insert”. The word alternatively is preferred to the word “alternately” (unless you really mean something that alternates).
* Do not use the word “essentially” to mean “approximately” or “effectively”.
* In your paper title, if the words “that uses” can accurately replace the word “using”, capitalize the “u”; if not, keep using lower-cased.
* Be aware of the different meanings of the homophones “affect” and “effect”, “complement” and “compliment”, “discreet” and “discrete”, “principal” and “principle”.
* Do not confuse “imply” and “infer”.
* The prefix “non” is not a word; it should be joined to the word it modifies, usually without a hyphen.
* There is no period after the “et” in the Latin abbreviation “et al.”.
* The abbreviation “i.e.” means “that is”, and the abbreviation “e.g.” means “for example”.

An excellent style manual for science writers is [7].

# Tool Process Testing and Validation

After the text edit has been completed, the paper is ready for the template. Duplicate the template file by using the Save As command, and use the naming convention prescribed by your conference for the name of your paper. In this newly created file, highlight all of the contents and import your prepared text file. You are now ready to style your paper; use the scroll

## Setup for Testing and Validation

**The template is designed for, but not limited to, six authors.** A minimum of one author is required for all conference articles. Author names should be listed starting from left to right and then moving down to the next line. This is the author sequence that will be used in future citations and by indexing services. Names should not be listed in columns nor group by affiliation. Please keep your affiliations as succinct as possible (for example, do not differentiate among departments of the same organization).

### For papers with more than six authors: Add author names horizontally, moving to a third row if needed for more than 8 authors.

### For papers with less than six authors: To change the default, adjust the template as follows.

#### Selection: Highlight all author and affiliation lines.

#### Change number of columns: Select the Columns icon from the MS Word Standard toolbar and then select the correct number of columns from the selection palette.

#### Deletion: Delete the author and affiliation lines for the extra authors.

## Validation Conditions

Headings, or heads, are organizational devices that guide the reader through your paper. There are two types: component heads and text heads.

Component heads identify the different components of your paper and are not topically subordinate to each other. Examples include Acknowledgments and References and, for these, the correct style to use is “Heading 5”. Use “figure caption” for your Figure captions, and “table head” for your table title. Run-in heads, such as “Abstract”, will require you to apply a style (in this case, italic) in addition to the style provided by the drop down menu to differentiate the head from the text.

Text heads organize the topics on a relational, hierarchical basis. For example, the paper title is the primary text head because all subsequent material relates and elaborates on this one topic. If there are two or more sub-topics, the next level head (uppercase Roman numerals) should be used and, conversely, if there are not at least two sub-topics, then no subheads should be introduced. Styles named “Heading 1”, “Heading 2”, “Heading 3”, and “Heading 4” are prescribed.

## DOE and its Variants

#### Positioning Figures and Tables: Place figures and tables at the top and bottom of columns. Avoid placing them in the middle of columns. Large figures and tables may span across both columns. Figure captions should be below the figures; table heads should appear above the tables. Insert figures and tables after they are cited in the text. Use the abbreviation “Fig. 1”, even at the beginning of a sentence.

1. Table Type Styles

| Table Head | Table Column Head | | |
| --- | --- | --- | --- |
| Table column subhead | Subhead | Subhead |
| copy | More table copya |  |  |

1. Sample of a Table footnote. (*Table footnote*)
2. Example of a figure caption. (*figure caption*)

Figure Labels: Use 8 point Times New Roman for Figure labels. Use words rather than symbols or abbreviations when writing Figure axis labels to avoid confusing the reader. As an example, write the quantity “Magnetization”, or “Magnetization, M”, not just “M”. If including units in the label, present them within parentheses. Do not label axes only with units. In the example, write “Magnetization (A/m)” or “Magnetization {A[m(1)]}”, not just “A/m”. Do not label axes with a ratio of quantities and units. For example, write “Temperature (K)”, not “Temperature/K”.

##### Result Discussion

The preferred spelling of the word “acknowledgment” in America is without an “e” after the “g”. Avoid the stilted expression “one of us (R. B. G.) thanks ...”. Instead, try “R. B. G. thanks...”. Put sponsor acknowledgments in the unnumbered footnote on the first page.

##### References

Capitalize only the first word in a paper title, except for proper nouns and element symbols.

For papers published in translation journals, please give the English citation first, followed by the original foreign-language citation [6].

**IEEE conference templates contain guidance text for composing and formatting conference papers. Please ensure that all template text is removed from your conference paper prior to submission to the conference. Failure to remove template text from your paper may result in your paper not being published.**

References

[1] A. Mayr *et al.,* "Electric Motor Production 4.0 – Application Potentials of Industry 4.0 Technologies in the Manufacturing of Electric Motors," in *2018 8th International Electric Drives Production Conference (EDPC)*, Schweinfurt, Germany, 2018, pp. 1–13.

[2] N. Boulanger *et al.,* "Aramid Based Slot Liners for Low Voltage Electric Motor Applications," in *2024 IEEE Electrical Insulation Conference (EIC)*, Minneapolis, MN, USA, 2024, pp. 17–21.

[3] Schaeffler ELMOTEC STATOMAT, *Slot Insulation Machines* (accessed: May 7 2025).

[4] Alliance Winding Equipment, *Slot Insulation Machines* (accessed: May 7 2025).

[5] GROB, *Slot Insulation Machine*.

[6] D. Mayer, L. Hausmann, N. Maul, L. Reinschmidt, J. Hofmann, and J. Fleischer, "Systematic Investigation of the Grooving Process and its Influence on Slot Insulation of Stators with Hairpin Technology," in *2019 9th International Electric Drives Production Conference (EDPC)*, Esslingen, Germany, 2019, pp. 1–7.